J Trauma Acute Care Surg. 2019 Jul;87(1S Suppl 1):S191-S196

# Lifesaving interventions in blackout conditions using night vision technology: Come to the dark side.

Derickson M, Kuckelman J, Phillips C, Barron M, Marko S, Eckert M, Martin M, Cuadrado D

BACKGROUND: During military combat operations and civilian night-time aeromedical transport, medical providers are frequently required to perform lifesaving interventions (LSIs) in low-light environments. Because definitive surgical care is often delayed until a white light environment is permissible, we sought to determine if night optical device (NOD) technology could enable surgical capabilities in blackout conditions.

METHODS: Using a crossover design, six surgeons performed 11 different procedures on six swine, three in normal light conditions (LC) and 3 in blackout conditions (BC) using two-chamber NODs after familiarization with the procedures in both conditions on manikins. Successful completion and procedural times were compared between groups.

RESULTS: Blackout conditions were confirmed with ambient light reading of 0.2 lux during BC versus 3962.9 lux for LC (p < 0.001). There were no significant differences in success rates for any procedure. There were no differences in operative times between BC and LC for extremity tourniquet placement, femoral artery cut-down and clamping, resuscitative thoracotomy, or percutaneous resuscitative endovascular balloon occlusion of the aorta placement. The following procedures took significantly longer in BC vs. LC: Focused Assessment with Sonography for Trauma examination (98 seconds vs. 62 seconds), peripheral IV placement (140 seconds vs. 35 seconds), intraosseous access (51 seconds vs. 26 seconds), jugular vein cut-down and access (237 seconds vs. 104 seconds), laparotomy and packing (71 seconds vs. 51 seconds), stapled splenectomy (137 seconds vs. 74 seconds), resuscitative endovascular balloon occlusion of the aorta placement via cutdown (1,008 seconds vs. 338 seconds), and cricothyroidotomy (177 seconds vs. 109 seconds) (all p < 0.05).

CONCLUSION: Lifesaving interventions can be safely and effectively performed in blackout conditions using NODs, although increased difficulty with select procedure types was identified. Focused training and technological improvements to currently available devices are needed.

LEVEL OF EVIDENCE: Basic science.