APPENDIX A: EXPOSURE REFERENCE LEVELS (ERL)

Exposure Limits between 100 kHz and 300 GHz radio frequency for Zone 0 and Zone 1. Zone 0 - unrestricted environments. Zone 1 - restricted to informed personnel with appropriate training. Zone 2 (not shown here) – restricted to specialized trained personnel and is allowed under unique circumstance only. All values are in root mean square (rms).

NOTE: Appendix A was reproduced according to the IEEE Standard C95.1-2345.3